r			

-SKINNING

FASTENER
-SPAN)

E WALL TRIM

RECEIVER TRIM (PR138)

1/8" RIVETS
@    12"   o.c.

DERLAYMENT NOT   BY  AEP-SPAN)

ER TRIM 38)

CUT AND PANEL UP 1"

UNDERLAYMENT
(NOT BY AEP-SPAN)		
	
REGLET TRI				

PANEL				

NOTE:				
	FIELD CUT FIRST				
	AND LAST PANELS				
	TO EQUAL WIDTH.				
	
CONSTRUCTION SEALANT (NOT BY AEP-S				
	3/8" BEAD NON-SKINNING				
	BUTYL SEALANT				
	ENGINEERED FASTENER				
	(NOT BY AEP-SPAN)				
	4" RG145 1				
	5"	RG147  \.._	REGLET TRIM				
	6"	RG149 J				

					
	B				

					

	SUBSTRATE	/				
	
PANCAKE HEAD				
	FASTENER				
	FASTENERS @ 12"	O.C.			

N
A Bluescope Steel Company
I...	DESIGN SPAN	HP
 	----...J1	SIDE WALL (RAKE WALL)	
		DS-11	

.)	
REV. 10/14/16