FIELD REQUI

SEAL ENDS OF PANELS

VALLEY SUP (NOT BY AEP

UNDERLAYMENT AEP-SPAN)

1"	MIN. AND POCKET
KINNING BUTYL OR TO
LE CLEAT

3/16"x7/8" BUTYL TAPE

@ 12

o.c.

FASTENERS

J	G
(J

ROO

3/16"x7/8" CONTINUOUS - BUTYL TAPE

PANCAKE HEAD FASTENERS
@ 12" o.c.

THERMAL  MOVEMENT	\

DESIGN SPAN	HP

VALLEY

\._

A Bluescope Steel Company
REV. 11/15/12

     L 	-.1)-1-

ind

DS-19
_)