Perception Collection®
(Vertical Installation) Installation Guide

Perception Collection®
(Vertical Install.) Installation Guide

- Table of Contents -

Section	Page

General Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	i
Panel Details	1
Clips	2
Panel Closures	3
Closure Installation	4
Base	5
Sill	6
End Wall . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	7
Outside Corner . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	8
Inside Corner	9
Soffit (Front)	10
Soffit (Back)	11
End Splice (w/Trim)	12
Parapet	13
Door/Window (Head)	14
Door/Window (Jamb)	15
Door/Window (Sill)	16
Wall Penetration (3D)	17
Wall Penetration	18
Rigid Insulation	19

©2017 ASC Profiles.  All rights reserved.	Jun17

General Notes
The attached installation details are intended to be a design aid and do not depict all situations. Modifications are the responsibility of the designer/user and should take into account climate conditions such as wind and snow, governing code requirements, and the actual usage and maintenance of the structure.

Applications:
Perception Collection can be utilized as a wall panel installed in the vertical or horizontal orientation. It shall not be utilized for roof applications. Perception Collection can be used over solid substrates or over spaced supports.
This installation guide depicts clip attached panels installed using flush mounted clips. Details for direct fastened panels or clip attached panels using standoff clips would be similar.

Flashings:
Where possible, flashings should be lapped away from prevailing winds. Certain flashings should be supported if it is likely that equipment (ladder, etc.) will be used against them. Check with AEP Span any time you intend to specify a prefinished flashing in a gauge or finish different than the Perception Collection. It is good practice to specify that all flashings be of the same material (gauge, color, finish) as the roof panels to ensure long-term durability. Field-painted flashings rarely equal the durability and colorfastness of factory baked-on paint systems. The enclosed details have minimized the use of exposed fasteners where possible. The edges of flashings have also been shown hemmed to strengthen and to minimize the exposure of cut edges.

Flashing design and fabrication is generally the responsibility of the contractor.  For convenience, we have provided some typical flashing drawings on our website at http://www.aepspan.com/roof/prodDetailad08.ht ml?id=35 . Applicable Perception Collection flashing part numbers are referenced within this installation guide. Note that flashing shapes and dimensions may vary greatly based on project requirements. Installation details and flashings referenced within are for general design guidance only.

Condensation, Insulation, & Ventilation:
It is the designer's responsibility to determine the need and composition of condensation control materials including insulation and vapor retarders, as well as ventilation requirements.
Metal wall products are susceptible to condensation and its control should be carefully considered.

Thermal Movement:
Both panels and flashings must allow for thermal movement (expansion and contraction) of the materials, especially where long lengths are used. Appropriate gaps or provisions must be provided to accommodate thermal movement.

Oil Canning:
Flat metal surfaces often display waviness commonly referred to as 'oil canning'. This can be caused by variations in raw material, processing variations, product handling, or variations in the installation substrate. Oil canning is a characteristic, not a defect, of panels manufactured from light-gauge metal. To reduce potential for oil canning, substrates should not deviate from a flat plane more than 1/4 inch in 20 feet, or 1/8 inch in 5 feet. Oil canning is not a cause for panel rejection. Additional technical information is available upon request.

References:
The Sheet Metal and Air Conditioning Contractors' National Association Inc. (SMACNA) manual is an excellent reference for sheet metal contractors. It’s guidelines for underlayments, gutter and downspout size requirements, and expansion/contraction of metals and flashing joints should be followed.

Technical Assistance:
Contact your AEP Span Sales Representative for additional information.

i

L -- 1·· 1·	21·	1'2 COVER-A-G1E&1· 1
PC10-12-	L 	I
t
11 ·,	i	5  •
PC20-12	L	I
i
PC30-12	L

PC40-12

i
PC50-12	L

PANEL  INTERLOCK	t 	
OPTIONS

DIRECT FASTENED (' D' P/N SUFFIX)

MATERIAL:
STEEL: 22 & 24GA (20GA NON-STD.) AVAILABLE LENGTHS: 5 ' -20'	
I

1		

CLIP ATTACHED ('C' P/N SUFFIX)	-
i
I--,	
                       N	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.		
PANEL DETAILS	
				                                       PCV-01	

REV. 6/15/17

):,	D
0
3•
0
):,	D
0
L_
L	2 1/2'

 FLUSH CLIP
P/ N: #WALLCLP

rr

/////		

9/32" DIA

t
7 /8'
t
9 / 16'

t

J

 INSTALLED POSITION	

Ir	

I	0
I
I
n-	4==-==---.,.)25)
:	0
I
I
I	0
I
LILl	)25)
I
I	0
I

 STANDOFF CLIP
P/ N: #WALLCL PO. 5	

N
I...		

L	PERCEPTION COLLECTION
VERTICAL INSTALL.			
CLIPS	
						PCV-02
.)	

r

CLPC-1P

TOP SIDE CLOSURE FOR ALL PANELS &
BOTTOM SIDE CLOSURE FOR PC1O-12

CLPC-2P

RE FOR PC4O-12 &

CLPC-3P

RE FOR PC2O-12 &

TEARO SECTIO
REVEALS AS REQUIRED

NOTE:	APPLICATIONS UTILIZING STANDOFF CLIP ALSO REQUIRE UNIVERSAL CLOSURE STRIP (AEP #CLEM1x19 . 68 OR EQUIV.) TO SEAL OFF ADDITIONAL 1/2" PANEL-TO-SUBSTRATE GAP.	

N
I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	
PANEL CLOSURES	
		PCV-03
.)	

r

TOP SIDE CLOSURE INSTALLATION

E

TOP

BOTTOM SIDE CLOSURE INSTALLATION
(FLUSH MOUNTED PANELS)

BOTTOM SIDE CLOSURE INSTALLATION
(PANELS WITH STANDOFF

BOTTOM	  
CLOSURE PLUG

1 X1 UNIVERSAL CLOSURE STRIP (AEP #CLEM1X19.68
OR EQUIV.)

- ---r::.r;/( :t::::: t---
NOTES:	- --=-:<,-·_;.;_ ,·	_.
•- :{ ,:.--_._ =-- ---
-    ALL  CLOSURE   PLUGS   SECURED   AND	··:.--:·i(/):   \ .
SEALED WITH POLYURETHANE SEALANT
(X) - NOT BY AEP SPAN	

I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	
CLOSURE INSTALLATION	
		PCV-04
.)	

REV. 6/15/17

r

TRIM
4"		DF026 DF027

DIM A
1  1/4"
1   3/4"

USAGE
FLUSH MOUNT
W/ 0 . 5" STANDOFF

1"
1/2"

. .·. 1
. .,
• I
. . . ·1
• ..•   ,I
.    .·.  1

. . ,
•_.•   II
••. .,I
--- 1
•-I
•   I

•. • .,I

SUBSTRATE
SPECIFIED UNDERLA YMENT (X) BUTYL FLASHING TAPE
(MAS . 025BF)

CLIP FASTENER

.     ·     1

. .,
.	•   •I I
°<. Il.l+,.\\
.    .·.   1
..    ,

PANEL CLIP

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

DRIP FLASHING

•   I
. .·. 1
•.• .,I

.4	41	4	2
<I	4
<I	4 ·

.

. <!.

. <I

.·.  1

t
4

(X) - NOT BY AEP SPAN

PERCEPTION COLLECTION
VERTICAL INSTALL.
L

BASE

PCV-05

)

r

.    .·   . 1
. I
••       I
. ..     ·1
.    .   I
..     I

.    .·.   1

: 1

• I
..	I

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)

....
..
..

1r1r
I
..I.
I

BUTYL FLASHING TAPE (MAS . 025BF)

CLIP FASTENER PANEL CLIP

<:\'.
.  .  I

..	I
..     I
.    .·.   1

INSIDE  CLOSURE  (SEALED  &
SECURED WITH  SEALANT) SILL  FLASHING  (V) ALTERNATE  WALL MATERIALS

..
. ..

.  . I I
·1

GAP

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS
PERCEPTION COLLECTION
VERTICAL INSTALL.
L

SILL

PCV-06

I...

..)

r							
				
3"			
				TRIM	DIM  A	DIM  B	USAGE			
				JT1O8	1  1/8"	1 1/8"	FLUSH MOUNT			
				A "		JT112	1  5/8"	1 1/2"	W/ 0 . 5" STANDOFF			
				B			

. .d	

SUBSTRATE			
				SPECIFIED UNDERLA YMENT (X)			
				CLIP FASTENER			

.d			
<I .	PANEL CLIP			
			·4				
			. ,.				
							
			<II '								
			4				
						<I					
			
.d	
.							
			
<I	
CONTINUOUS BEAD OF NON­			
			
_	
.d				SKINNING BUTYL TAPE OR SEALANT			
				TRIM FASTENER W/SEALING WASHER			
				OR RIVET AT 12 " O.C. MAXIMUM			
				J  TRIM			
				SEALANT/ BACKER ROD			

(X)	

-	

NOT BY AEP SPAN				

I...	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.	
END WALL	
				PCV-07	

.)	

r				

DIM  A	USAGE
7/8"	FLUSH MOUNT
1   3/8"	W/ O. 5" STANDOFF

>•• >I" I
••	I
. I
•    I
•.       I
.    .·   . 1
•   I
••	I
.· ·1
I
. I_

<!.I, '\.
:·I
.   I
I
I+
 	      • LI	
		1/2"f			
		
1 1/4"	
1 1/2"
A
4"	TRIM ZC225 ZC228		
		1/	1/2"	1 1/2"		
		1/8'	I--	1/2"			
		JC096	4"			
		OC111			

STARTER	

CLEAT (JCO96)			
		SUBSTRATE			
		SPECIFIED UNDERLA YMENT (X)			
		CLIP FASTENER			
		PANEL CLIP			

 			
		_•      .  •/.  ·      .  ·      .  ·      .  ·      .  ·      .	.  ·      .  ·      .	.  ·      .  ·      .  ·      .  ·      .  •      .  •      .  ·      .  ·			

CONTINUOUS BEAD OF NON­			
		SKINNING BUTYL TAPE OR SEALANT			
		TRIM FASTENER W/SEALING WASHER			
		OR RIVET AT 12" O.C. MAXIMUM			
		Z-METAL			
		OUTSIDE CORNER TRIM (OC111)			
	(X)	- NOT BY AEP SPAN			

N
I...	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.		
OUTSIDE CORNER	
				PCV-08
..)	

r		1    1l/4"	

1/2"

4"

4"

,; 	
1/2" l	IC093

=	. . . . . . . . . . . .

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)
. ..    · 'I
STARTER CLEAT (JCO96)
. .. ·1
I	INSIDE CORNER TRIM (ICO93)
· .. .·1. '
> 1-I
.	·,
EALING WASHER
'"'	C. MAXIMUM
OF NON-
I	SKINNING BUTYL TAPE OR SEALANT
1	
		1/ 	1/2"		
		1/8'	I--		
		JCO96		

=			

				

(X) -	

NOT BY AEP SPAN		

N
I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	
INSIDE CORNER	
		PCV-09
..)	

r	

TRIM	DIM  A	USAGE
DFO32	1  1/8"	FLUSH MOUNT
4"	DFO33	1  5/8"	W/O.5" STANDOFF

135" A
c/1/2"
OPEN HEM

1- :-
I •
I ••
I :
I .
I    •
SUBSTRATE	I >
I    •
I ••
SPECIFIED   UNDERLA YMENT  (X)	J>
I .
BUTYL  FLASHING  TAPE	I
(MAS . O25 BF)
I
PANEL  CLIP	I .
CLIP FASTENER	I
INSIDE  CLOSURE  (SEALED  &
SECURED  WITH SEALANT)

DRIP FLASHING
\\\\\\\
tr'
I
L.. .  . .  . .  . .  . .
I .

--	,;-..
1/4	 	
t

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

. .	

(V)	1/2"
1/2"
/135·

COVER TRIM

. .  .   .   .   .   -.   .   .  ·.··.  .  ·.  ·.  ·.
.	.	.     .  .   .	. . . .

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF  NON- SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM
COVER TRIM (V)	
	_E	PERCEPTION COLLECTION	
SOFFIT (FRONT)	

I...	8N	VERTICAL INSTALL.
L		
			PCV-10
..)	

r									
					1/2"				
				4"					
		
4"							
		1/2" l		
IC093					
		
- .  ----.   .    .   .  ·.!.    .   .	.  -·-.   .  ·..  .  ·     .					

ij 	,,
7 : :			
									
						I    .			
						I .  ;;,. 1			
		INSIDE CORNER TRIM (ICO93)							
		POINT OF FIXITY FASTENER ;							
		2 PLACES MIN. AT TOP OF PANEL							
		SPECIFIED UNDERLA YMENT (X)							
		SUBSTRATE							
		TRIM FASTENER W/SEALING WASHER							
		OR RIVET AT 12 " O.C. MAXIMUM							
		CONTINUOUS BEAD OF NON­							
		SKINNING BUTYL TAPE OR SEALANT							
		OUTSIDE CLOSURE (SEALED &							
		SECURED WITH SEALANT)							
		OPTIONAL FIELD FABRICATED							
		CLOSURE COVER TRIM (X)							
		CLIP FASTENER							
		PANEL CLIP							

(X)	

- NOT BY AEP SPAN							

I...		

L	PERCEPTION COLLECTION
VERTICAL INSTALL.	
SOFFIT (BACK)	
				
	PCV-11	

.)	

r					

TRIM	DIM  A	USAGE
HTO92	1  1/8"	FLUSH MOUNT HT103	1  5/8"	W/O.5" STANDOFF

1 1/2"

SUBSTRATE
....   I
SPECIFIED UNDERLA YMENT (X)
. . I I
·1!'-il-	BUTYL FLASHING TAPE
(MAS . O25 BF)
1 I
'1""	PANEL CLIP
I
CLIP FASTENER

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)
END SPLICE /SILL FLASHING POINT OF FIXITY FASTENER;
2 PLACES MIN . AT TOP OF PANEL
•••       I
..        1	---

I
••	I
••       I
.. I	TRIM FASTENER W/SEALING WASHER
..
OR RIVET AT 12" O. C. MAXIMUM

OUTSIDE CLOSURE (SEALED &
SECURED  WITH SEALANT)

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)		

4"			
				
A			
				1/2" l			

=				

(X)	

-		

NOT BY AEP SPAN			

I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	
END SPLICE (W/TRIM)	
		                                      PCV-12	

.)	

r			
	
1 1/ 2"		
	135'		
	5/8"		
	TC209		

PARAPET FLASHING (V)		
			
	POINT OF FIXITY FASTENER;		
	2 PLACES MIN. AT TOP		
	OF  PANEL		
			
	TRIM CLEAT		
	TRIM FASTENER W/SEALING WASHER		
	OR RIVET AT 12" O. C. MAXIMUM		
	CONTINUOUS BEAD OF NON­		
	SKINNING BUTYL TAPE OR SEALANT		
			
	OUTSIDE CLOSURE (SEALED &		
	SECURED WITH SEALANT)		
	OPTIONAL FIELD FABRICATED		
	CLOSURE  COVER TRIM (X)	I		
	I .		
	PANEL CLIP		
	CLIP FASTENER		
	SPECIFIED		
	UNDERLA YMENT (X)		
	SUBSTRATE		

(X)	-	NOT BY AEP SPAN		
	(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS		

I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	
PARAPET	
		PCV-13
..)	

r				

TRIM	DIM A
4"	HTO93	1  1/ 8 "
HT102	1  5 / 8 "

A	1/ 2"
135"	4"	135

I
I:     :-       1
I     . ,    I I
I
I	I
I	I
I   .,	I
I	I
I
. ,I
I
.... I
I
. ,	I

.  . I I

<'.\ ' '.
••	I
••	I
.     .·        . 1
. ,I
•   •	I
.  .. ·1
•   •	I
1	. ,	I
I
 	 	7			
					
USAGE		
					FLUSH MOUNT		
					W/ O. 5 " STANDOFF		

1/2"				

I				
			I				
			I				
			I				
			I				
			I				
			I				
			I				
			I				
			I				
			I
I		SUBSTRATE		
			I
I		SPECIFIED UNDERLA YMENT (X)		
			I
I I		BUTYL FLASHING TAPE (MAS . O25 BF)		
			I
I		CLIP FASTENER		
			I				
			I I		PANEL CLIP		
					INSIDE CLOSURE (SEALED &		
					SECURED WITH SEALANT)		
					HEADER TRIM		
			l					

( X)	

-	

NOT BY AEP SPAN				

I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	DOOR / WINDOW (HEAD)	
		                                      PCV-14	

.)	

r		

1/2"
TRIM	DIM  A	USAGE
135'	1  1/2"	ZC225	7/8"	FLUSH MOUNT
A	ZC228	1  3/8"	W/O.5" STANDOFF

4"	1  1/2"	--------
, ,
1/2"	I
I
1  1/2"	I
\
WC217	I
I
 	 	I
I
I
/

ALTERNATE DETAIL

SUBSTRATE SPECIFIED UNDERLA YMENT (X)
CLIP FASTENER PANEL CLIP

ZEE FLASHING CONTINUOUS   BEAD   OF NON­
SKINNING  BUTYL  TAPE  OR  SEALANT

TRIM FASTENER W/SEALING WASHER OR  RIVET  AT 12"   O. C. MAXIMUM

WALL  CLOSURE  (WC217)

- NOT BY AEP SPAN			

SEALANT		
			TRIM ANGLE		
			WALL CLOSURE		
			
]		

(X)				

N
I...	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.	DOOR / WINDOW (JAMB)	
				PCV-15	

.)	

r			

1/2"
135·

4"

1/2"

1 1/2" WC217

L	J	l J 
----f---7
•  I
.               ·1

<11\\111
••      I
.  .  ·.  1
•  I
.               ·1
.	I.
1"'
.        ·1
>j
•  I
.                  ·   1
·· ·1
.                     ·    1
•  I
. ..  · 1

NOT BY AEP SPAN			

WALL CLOSURE (WC217)		
				
TRIM FASTENER W/SEALING WASHER		
				OR RIVET AT 12" O.C. MAXIMUM		
				CONTINUOUS BEAD OF NON­		
				SKINNING BUTYL TAPE OR SEALANT		
				OUTSIDE CLOSURE (SEALED &		
				SECURED WITH SEALANT)		
				OPTIONAL FIELD FABRICATED		
				CLOSURE COVER TRIM (X)		
				POINT OF FIXITY FASTENER;		
				2 PLACES MIN. AT TOP OF PANEL		
				
PANEL CLIP		
				CLIP FASTENER		
				SUBSTRATE		
				SPECIFIED UNDERLA YMENT (X)		

(X)	

-				

I...	PERCEPTION COLLECTION
VERTICAL INSTALL.
L	DOOR / WINDOW (SILL)	
		                                       PCV-16	

.)	

r		

......
......
......
'-....'-........._	......
...... ......	......
......
'-...................    ......
......	......
......	',
'-................	'1
'	I
>
' ...... ......
......_ ',
...... ......
'

SEAL PERIMETER OF FLASHINGS AND ALL TRIM OVERLAPS WITH A CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT
OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)		

DRIP FLASHING			
	TRIM FASTENER W/SEALING			
	WASHER, OR RIVET			
	SEALANT			
	OVERLAP UPPER/LOWER			
	FLASHINGS			
	WALL PENETRATION			

				

	
(X) - NOT BY AEP SPAN			

I...	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.	
WALL PENETRATION (3D)	
			PCV-17	

.)	

REV. 6/15/17

r				

SPECIFIED UNDERLA YMENT (X)			
	SUBSTRATE DRIP FLASHING (V)			
	CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT UNDER COVER PERIMETER			
	SEAL PENETRATION PERIMETER WITH POLYURETHANE SEALANT			
	WALL PENETRATION			
	OVERLAPPED PENETRATION COVER

PROVIDE SUFFICIENT CLEARANCE BETWEEN FLASHING & PENETRATION TO ACCOMODATE  THERMAL MOVEMENT

TRIM  FASTENER W/SEALING
WASHER  OR RIVET	-,--
1
I I I I I I I
I		
	OUTSIDE CLOSURE (SEALED &
SECURED  WITH SEALANT)			
	OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)			

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS			

I...	

L	PERCEPTION COLLECTION
VERTICAL INSTALL.	
WALL PENETRATION	
			                                       PCV-18	

.)	

r

H

SUBSTRATE	  

RIGID  INSULATION (X)

SPECIFIED UNDERLA YMENT (X)

CLIP FASTENER PANEL CLIP
ZEE FLASHING (V)

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS AND GAGE VARY BASED ON PROJECT CONDITIONS
PERCEPTION COLLECTION
VERTICAL INSTALL.
L

RIGID INSULATION

PCV-19

I.	)

MANUFACTURING FACILITY:

Anchorage, Alaska
2441 Cinnabar Loop
Anchorage, AK 99507
Alaska Customer Service: 904-267-3004

Fontana, California
10905 Beech Avenue
Fontana, CA 92337

CORPORATE HEADQUARTERS:

ASC Profiles LLC 2110 Enterprise Boulevard West Sacramento, CA 95691

CUSTOMER SERVICE:
800-733-4955

Visit us at:
www.aepspan.com

©2017 ASC Profiles LLC.  All rights reserved.